{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["模温机日常点检表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"模温机日常点检表","index":0,"n_rows":25,"n_cols":36,"rows_kept":25,"merged":[[0,0,0,1],[0,3,2,23],[0,24,0,29],[0,30,0,35],[1,0,1,1],[1,24,1,29],[1,30,1,35],[2,0,2,1],[2,24,2,29],[2,30,2,35],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,3,35],[10,0,11,0],[10,1,11,1],[10,2,11,2],[10,3,11,3],[12,0,13,0],[12,1,13,1],[12,5,12,12],[12,13,12,20],[12,21,12,28],[12,29,12,35],[13,5,13,35],[14,5,14,12],[14,13,14,20],[14,21,14,28],[14,29,14,35],[15,5,15,35],[16,5,16,35],[17,0,18,3],[19,0,19,1],[19,3,19,20],[19,21,19,28],[19,29,19,35],[20,0,20,1],[20,3,20,20],[20,21,20,28],[20,29,20,35],[21,3,21,20],[21,21,21,28],[21,29,21,35],[22,3,22,20],[22,21,22,28],[22,29,22,35],[23,3,23,20],[23,21,23,28],[23,29,23,35],[24,0,24,35]],"flags":["formulas_cached_only"]}
["日    期",null,null,"模  温  机  日  常  点  检  表",{"$nulls":20},"编    号",{"$nulls":5},"MWJ-02"]
["设备型号",{"$nulls":23},"修改次数",{"$nulls":5},"第1次修改"]
["设备编号",{"$nulls":23},"发布日期",{"$nulls":5},"2017-12-10"]
["项次","检查维护保养项目","点检标准","点检及保养措施","周期","     点        检        保         养         结         果"]
[{"$nulls":5},1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31]
[1,"控制线路","导通良好、无松动","检查、紧固","1次/日"]
[2,"管路","无堵塞现象","清理、疏通","1次/日"]
[3,"泵浦","无异音、无剧烈震动","检查、保养、紧固","1次/日"]
[4,"阀门","无漏水（油）","检查、修理、更换","1次/日"]
[5,"分流板与模具连接部位,冷却水入/出水口","连接状态检查","连接是否到位，水管有无收缩、膨胀造成漏水，如漏水及时更换","1次/日"]
[6,"控制面板","设定温度和实际温度温差在正负五度之内","检查、调整、更换并记录温度","设定"]
[{"$nulls":4},"实际"]
[7,"过滤器","清理过滤器","使用专用工具，进行清理","1次/周"]
[null,null,"定期更换过滤器","每季度进行更换","1次/季度"]
[8,"泵漏水（油）检查","无泄露现象","确认泵出入口有无损坏，有无漏水（油）","1次/周"]
[9,"温度及液位感应器","无断线及接触状态","温度感应器的阻力值（Ω）0.2-0.3以上，KΩ或MΩ时为烧损状态","1次/季度"]
[10,"机器内部检查","无黑色粉尘","关闭CONTROL DOOR确认在机器内部的MAGNETIC表面有无粉尘，粉尘多需更换","1次/半年"]
["良好○异常X并做好详细记录                                                    ",{"$nulls":3},"检查"]
[{"$nulls":4},"审核"]
["日期",null,"故障内容","故障原因及采取的措施",{"$nulls":17},"完成日期",{"$nulls":7},"维修者"]
[]
[]
[]
[]
["南京欧能机械有限公司400-000-9261"]